桁架单点吊机

桁架尺寸：1500\*600\*600mm

电机功率：7.5KW（伺服电机）

输出转速：259r/min

输出扭矩：267Nm

卷筒直径：200mm（改成180）

钢丝绳直径：7mm

控制方式：PLC+触摸屏，通信协议：profinet

载荷：250KG

速度：2.4m/s

自重：280KG

Single point winch

Dimension: 1500\*600\*600mm

Power: 7.5KW (servo motor)

Output speed: 259r/min

Output torque: 267Nm

Drum diameter: 200mm

Wire diameter: 7mm

Control mode: PLC + touch screen

Communication protocol: profinet

Load capacity: 250KG

Speed: 2.4m/s

Dead weight: 280KG

K/F单层卷绕提升机

型号：BRD-K-Y-77-58.34-3-950-6-0.300-1.3-245

电机功率：2.2-15KW（YEJ系列双制动电机）

卷筒直径：200/245/275/320mm

钢丝绳直径：6mm /7mm /8mm /10mm

控制方式：手动/ PLC+触摸屏

通信协议：profinet

吊点数：1-8（可定制）

载荷：400-1500KG（可定制）

速度：0.366-0.448m/s

自重：150-450KG（根据定制设备确定）

K/F winch

Model NO：BRD-K-Y-77-58.34-3-950-6-0.300-1.3-245

Power: 2.2~15KW (YEJ series double brake motor)

Drum diameter: 200/245/275/320mm

Wire diameter: 6mm /7mm /8mm /10mm

Control mode: manual/ PLC + touch screen

Communication protocol: profinet

Number of points: 1~8 (customized)

Load capacity: 400 ~1500KG (customized)

Speed: 0.366 ~ 0.448m/s

Dead weight: 150 ~ 450KG

RV单层卷绕提升机

BRD-RV-Y-110-40-2.2-400-6-0.366-1.3-200

电机功率：2.2-5.5KW（YEJ系列制动电机）

卷筒直径：200/245mm，

钢丝绳直径：6mm /7mm

控制方式：手动/ PLC+触摸屏

通信协议：profinet

吊点数：1-8

载荷：400-900KG

速度：0.366-0.448m/s

自重：150-320KG

RV winch

BRD-RV-Y-110-40-2.2-400-6-0.366-1.3-200

Power: 2.2~5.5KW (YEJ series brake motor)

Reducer: RV110/130/155

Reduction ratio: 40:1/ 50:1/ 60:1

Drum diameter: 200/245mm

Wire diameter: 6mm /7mm

Control mode: manual/ PLC + touch screen

Communication protocol: profinet

Number of points: 1~8

Load capacity: 400 ~900KG

Speed: 0.366 ~ 0.448m/s

Dead weight: 150 ~ 320KG

多层叠绕提升机

BRD-RV-D-110-40-2.2-600-4-0.256-1.5

电机功率：1.5-4.0（YEJ系列制动电机）

卷筒直径：起始层140mm，

钢丝绳直径：4.2 mm / 5.1mm

控制方式：手动/ PLC+触摸屏

通信协议：profinet

吊点数：1-7

载荷：200-600KG

速度：0.3m/s

自重：45-140KG

BRD-RV-D-110-40-2.2-600-4-0.256-1.5

Power: 1.5~4.0KW (YEJ series brake motor)

Reducer: RV75/90/110

Reduction ratio: 25:1/ 30:1/ 40:1/ 50:1

Drum diameter: 140mm

Wire diameter: 4.2 mm / 5.1mm

Control mode: manual/ PLC + touch screen

Communication protocol: profinet

Number of points: 1~7

Load capacity: 200 ~600KG

Speed: 0.3m/s

Dead weight: 45~ 140KG

F自排绳单点吊机

电机功率：2.2-15KW（YEJ系列制动电机，可定制伺服电机）

卷筒直径：245mm-320mm

钢丝绳直径：5.1-10mm

控制方式：手动 /PLC+触摸屏

通信协议：profinet

吊点数：1-7

行程8m（可定制）

载荷：250-1500KG

速度：0.1-1.5m/s

自重：75-500KG

F single point winch

Power: 2.2-15KW (YEJ series brake motor, servo motor can be customized)

Reducer: F

Drum diameter: 245mm-320mm

Wire diameter: 5.1-10mm

Control mode: manual/ PLC + touch screen

Communication protocol: profinet

Number of points:1-7

Travel: 8m ( can be customized)

Load capacity: 250-1500KG

Speed: 0.1-1.5m/s

Dead weight: 75-500KG

拉幕机

电机功率：0.3-2.2/KW

速度： 0.01~1m/s (可调速)

行程：最大20m (可定制)

承重：100~600KG (可定制)

Draw Curtain Machine

Motor power: 0.37-2.2/KW

Curtain moving speed: 0.01~1m/s (adjustable)

Travel: 8m (can be customized)

Load capacity: 100~600KG (can be customized)

Product name: